**Breaking Down A-TOMATO-FLAMES**

* A – Airspeed Indicator
* T – Tachometer (for each engine)
* O – Oil Pressure Gauge (for each engine)
* M – Manifold Pressure Gauge (for each engine, if applicable)
* A – Altimeter
* T – Temperature Gauge (for each liquid-cooled engine)
* O – Oil Temperature Gauge (for each engine)
* F – Fuel Gauge
* L – Landing Gear Position Indicator (if applicable)
* A – Anti-Collision Lights (For aircraft certificated after March 11, 1996)
* M – Magnetic Compass
* E – Emergency Location Transmitter (ELT)
* S – Safety Belts